# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:** **Public procurement of supplies for project REBIOFORESTS**

**Ref. number:** **HR-RS00062 – PP2 – TD02**

**LOT 3 - Mulcher**

**Columns 1-2 should be completed by the Project partner**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the Contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the Project partner shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words “compliant” or “yes” are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

The requirements set out in the technical specifications represent the minimum technical characteristics which offered goods must satisfy, unless stated otherwise, and tenderers are not allowed to modify technical specification in any way.

For each item for which it is not explicitly stated that it is allowed to offer goods of the equal characteristics, i.e. for each item where it is not stated “or equivalent”, for the purposes of this tender documentation it is assumed that words “or equivalent” are stated, and tenderer is allowed to offer equivalent goods / goods of equivalent characteristics.

**General Requirements**

• All requirements stated and outlined in this document must be regarded as mandatory and the minimum acceptable criteria. All requirements outlined in this document are accompanied by the phrase "or equivalent".

• The tenderer is required to provide the specifications of the offered items in the Technical Offer, including details such as the manufacturer, product type, model, and country of origin. All documentation must be provided in English or Serbian, both in hardcopy and electronic formats.

• The selected contractor is required to provide all necessary documentation for the registration of the completed vehicle in accordance with the relevant legal regulations in the Republic of Serbia. This includes the Certificate from the Agency for Traffic Safety confirming the vehicle examination, as well as the technical inspection registration sheet, which is required for further vehicle registration.

| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s decision (Y/N)** |
| --- | --- | --- | --- | --- |
| **1** | **Mulcher**  **Quantity: 1 Unit**  **(Forest Multchercutters with the ability to crush underground roots and stumps up to 30 cm, working depth up to 30 cm. A professional machine with a fixed working tool intended for hanging on tractor power 120-160 hp)** |  |  |  |
|  | **Required technical characteristics:**  • Min 595 mm diameter rotor with fixed working tools placed in a spiral  • Working reach 1840 mm  • Weight of the chipper: Max 2260 kg  • Number of working tools: Min 66+4 pieces  • Diameter of wood grinding: Min 30cm  • Diameter of stumps for grinding: Min 30 cm  • Working depth up to 30 cm  • Adjustable hardox counter knives  • Housing made of HARDOX with reinforced inner walls  • Drive – direct transmission with freewheel  • Friction clutches - overload protection  • Cardan shaft with lamellas  • Hydraulic rear door  • Hydraulic hoses integrated in the housing  • Protective chains  • Hydraulic top link  • Hydraulic rear roller for regulating the working depth |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: “Forest Administration” Višnjićevo, Radnička br. 2, Višnjićevo, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |

**<Signature of authorised representative of the legal entity >**

**< Name and position of authorised representative of the legal entity >**

**< Date >**