# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:** **Public procurement of supplies for project REBIOFORESTS**

**Ref. number:** **HR-RS00062 – PP2 – TD02**

**LOT 5 - SUV vehicle**

**Columns 1-2 should be completed by the Project partner**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the Contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the Project partner shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words “compliant” or “yes” are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

The requirements set out in the technical specifications represent the minimum technical characteristics which offered goods must satisfy, unless stated otherwise, and tenderers are not allowed to modify technical specification in any way.

For each item for which it is not explicitly stated that it is allowed to offer goods of the equal characteristics, i.e. for each item where it is not stated “or equivalent”, for the purposes of this tender documentation it is assumed that words “or equivalent” are stated, and tenderer is allowed to offer equivalent goods / goods of equivalent characteristics.

**General Requirements**

• All requirements stated and outlined in this document must be regarded as mandatory and the minimum acceptable criteria. All requirements outlined in this document are accompanied by the phrase "or equivalent".

• The tenderer is required to provide the specifications of the offered items in the Technical Offer, including details such as the manufacturer, product type, model, and country of origin. All documentation must be provided in English or Serbian, both in hardcopy and electronic formats.

• The selected contractor is required to provide all necessary documentation for the registration of the completed vehicle in accordance with the relevant legal regulations in the Republic of Serbia. This includes the Certificate from the Agency for Traffic Safety confirming the vehicle examination, as well as the technical inspection registration sheet, which is required for further vehicle registration.

| **1.**  **Item Number** | **2.**  **Specifications Required** | **3.**  **Specifications Offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation Committee’s decision (Y/N)** |
| --- | --- | --- | --- | --- |
| **1** | **SUV vehicle**  **Quantity: 1 Unit** |  |  |  |
|  | **Required technical characteristics:**  **Body type:** SUV, 5 Doors, 5 Seats   * Length: from 4300 to 4400 mm * Width: from 1800 to 1820 mm * Height: from 1660 to 1700 mm * Wheelbase: from 2600 to 2700 mm * Ride height (ground clearance): from 210-220 mm * Trunk (boot) space: from 440 to 460   **Engine:** from 1149 to 1199 cm3  **Power:** from 95 to 99 kw / 130 Hp, 230 Nm  **Fuel:** Petrol (Gasoline)  **CO2 emissions (WLTP):** from 129 to 139 (g/km)  **Number of cylinders:** 3  **Drive wheel:** All wheel drive (4x4)  **Number of gears and type of gearbox:** 6 gears, manual transmission  **SAFETY AND DRIVING ASSISTANCE** Emergency Braking Assistance System (AFU) Lane Keeping Assist System (LKA) Anti-lock Braking System (ABS) Hill Start Assist (HSA) Electronic Stability Control (ESP) Emergency Call System Driver Fatigue Warning System Forward Collision Warning System Automatic Emergency Braking with Pedestrian and Cyclist Detection Side Airbags and Curtain Airbags Front Airbags for Driver and Passenger Automatic Activation of Warning Lights in Case of Collision or Sudden Braking Passenger Airbag Deactivation Cruise Control and Speed Limiter Remote Central Locking Height-adjustable Seat Belts Seat Belts with Pretensioner and Force Limiter Reverse Driving Light Indirect Tire Pressure Monitoring System Brake Protection from Foreign Particles Third Brake Light Seat Belt Reminder (for all seats) Rear Center Three-point Safety Belt ISOFIX System for Rear Child Seat Attachment Particulate Filter ECO Driving Mode Gear Shift Indicator Traction Control System Rearview Camera Front Fog Lights Automatic High/Low Beam Activation  **COMFORT** Heated Rear Window Electrically Adjustable and Heated Exterior Mirrors Power Front Windows Driver’s Seat Height Adjustment 1/3 - 2/3 Split-folding Rear Bench Side Turn Indicators on Exterior Mirrors Headrests on All Seats Height- and Depth-adjustable Steering Wheel Phone Holder Rain-sensing Wipers Power Rear Windows Center Console with Armrest and Storage Space All-season Tires (for 4x4 Only) Automatic Climate Control with Temperature Sensor Electrically Foldable Exterior Mirrors Driver's Seat with Lumbar Support 12V Power Outlet Front and Rear YouClip 3-in-1 Box  **DESIGN** Body-colored roofSynthetic leather steering wheelBody-colored bumpersModular roof rails with copper-colored detailsExtra tinted rear windowsCopper-colored exterior mirrorsBody-colored exterior door handles17" aluminum wheels with semi-diamond shineVentilation outlet frames in a "Y" shape with copper-colored detailsSide panels in "Y" shape in Lichen Kaki colorRubber floor mats Rubber trunk mat  **MULTIMEDIA** Min 7" TFT information screen between the gauges 4G network connectivity  **TECHNICAL DETAILS**  Vehicle type: passenger - off-road  Fuel type: petrol  Engine generation: Euro 6  Transmission: manual 6-speed  Drive: 4\*4 (front and rear)  Number of doors: 5 (five)  Number of seats: 5 (five)  Body color: METALLIC GREEN  Engine displacement: Min 1199 cm3  Engine power: Min 96 kW  **ADDITIONAL OPTIONS**  Driving package  Multiview camera  Front and rear parking sensors  Blind spot monitoring system  Multimedia package  Multimedia MEDIA DISPLAY with Min 10” touch screen with DAB, Bluetooth, USB and AUX functions with 6 speakers  Automatic handbrake  Wireless phone charging  18” aluminium wheels  Spare wheel |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **All items** | **Delivery** of all items to following address: Public Enterprise “VOJVODINAŠUME”, Preradovićeva 2, 21131 Petrovaradin vo, Republic of Serbia. |  |  |  |
| **All items** | **Testing** of all basic functions of the instrument on a set of producers standard samples commonly used for the corresponding instrument.  Installed equipment must be tested as system, compatible with existing system. |  |  |  |
| **All items** | Technical documentation for equipment (Operating manuals/ Users Guide/ Equipment operating instructions/ Cleaning procedures/ Maintenance procedures/ Calibration procedures) upon delivery. |  |  |  |
| **All items** | **Warranty**  Warranty period 365 days from the issuance of PAC (Provisional Acceptance Certificate) in accordance with article 32 SC and GC of the Contract. Offer must include warranty service description including:   * Service organisation contact data including name, postal address, telephone number, fax number and e-mail address; * Guaranteed that any requests for services will be attended to within 48 hours; * Guarantee that all items can be repaired or alternatively replaced within a maximum of 7 days; * Letter of confirmation that genuine spare parts and consumables will be available for a period of minimum 3 years from the date of final acceptance of the equipment. |  |  |  |
| **All items** | **Commercial warranty**  365 days from the issuance of FAC (Final Acceptance Certificate) in accordance with the conditions laid down in Article 32 of the General Conditions and Article 33 of the Special Conditions.  Detailed description of the organisation of the proposed service and description of the Manufacturer’s commercial warranty shall be included in the offer. |  |  |  |

**<Signature of authorised representative of the legal entity >**

**< Name and position of authorised representative of the legal entity >**

**< Date >**